FMTK – Finitron Multi-Tasking Kernel

All FMTK functions return a status in $v0 which is normally E\_Ok if the function performed successfully. A second return value is return in $v1 for some functions.

Arguments to FMTK functions are passed in a1 to a6. The function call number is specified in a0.