# FT64v3 ISA

## Overview

The FT64v3 ISA is in part organized around the idea of a simple compiler at the expense of some hardware cost. The ISA makes use of a unified register file for integer and floating-point registers. This makes it a bit easier to manage register usage by the compiler. Having a large number of registers directly available means the compiler doesn’t have to be as sophisticated in it’s allocation of registers and good performance is still possible. However, increasing the number of bits required to represent registers leads to an increase in the size of instructions.

This instruction set uses a fixed 36-bit format instruction as its base because 32 bits isn’t quite enough. 36 bits may seem like an odd number, but the number of bits in an instruction is somewhat irrelevant as long as all instructions can fit on a cache line. Instruction caches are loaded in terms of cache lines. Sixteen 36-bit instructions will fit into a 576-bit cache line with no wasted space. 576 bits is 72 bytes, in range with typical cache line sizes. It is also a multiple of 64 bits, the width of the data bus.

## Design Considerations

### Compression

A number of contemporary processors make use of compressed instructions sets to improve code density as a way to compete with other designs using byte codes. Narrower instructions make better use of memory and caches. They have benefits in the form of performance and power consumption. They are so important to contemporary designs that RiSC-V for instance reserves three quarters of the opcode space for compressed instructions. Other processors have mode switching instructions to enable compressed instruction sets. This design directly supports compressed instructions; one half of the instruction space is allocated for compressed instructions. Half of the compressed instruction space is reserved for memory operations, the other half for other operations.

Typically, a compressed version of the instruction set relates to the uncompressed version in terms of registers used and field specifications. The register and field specifications map more or less directly to fields in the expanded instruction. The mapping is designed to take a minimal amount of logic to convert into expanded instructions so that the decompression doesn’t significantly impact the cycle time of the processor. A subset of registers may be supported along with a subset of operations that the processor provides.

Significant analysis has gone into which instructions should be available in a compressed form. It is often the same subset of instructions that are best compressed. These instructions typically include an add of a small amount to a register, and frame pointer or stack pointer relative loading / store instructions.

For this design, rather than develop a format for and completely specify fields for compressed instructions, compressed instructions are simply expanded from look-up tables. An application profiler may be used to select the set of instructions to compress. The compressed instruction set in use is definable at run-time, similar to a micro-code update capability. Using lookup tables may reduce the number of compressed instructions available, but the best selection for a given app(s) can be chosen. Decompressing instructions becomes a simple indexed table lookup rather than logic.

A parcel size one half of the chosen base instruction size or 18-bit parcels offer good compression. Compressed instructions use a 8k entry lookup table to decompress the instructions. It is envisioned that decompressing these instructions may require an extra clock cycle for access to the lookup table. Often the instruction will be able to queue in the pipeline without knowing the exact details of the instruction. Looking up the instruction is similar to having to fetch values from the register file. The exact opcode can be filled in a cycle later after lookup takes place.

A consequence of the delay in decompressing an instruction is that a compressed branch type instruction may have an additional clock cycle of delay causing a reduction in performance.

# Instruction Set Description

## Overview

This instruction set uses a fixed 36 bit format instruction as its base. 36 bits may seem like an odd number, but the number of bits in an instruction is somewhat irrelevant as long as all instructions can fit on a cache line. Instruction caches are loaded in terms of cache lines. Sixteen 36-bit instructions will fit into a 576-bit (72 byte) cache line with no wasted space and it’s a multiple of 64 bits. Part of the reason for a 36-bit base instruction is that 32 bits isn’t quite enough. This is brought about because of the desire for a base of 64 available general-purpose registers in the instruction set and the desire to support a full instruction set. 64 registers were chosen because it makes the compiler simpler to implement. There is no distinguishing between integer and floating-point register sets.

## Instruction Addresses

Instructions are addressed in 36-bit parcels as if they were composed of two eighteen-bit parcels. An 18-bit parcel size is to allow for a compressed instruction set. In order to keep instruction addresses and data addresses the same, instruction addresses are represented with a two bit fractional portion.

## Formats

Instructions have a fixed 36 bit format. There are only a handful of different instruction formats. The opcode, register read Ra, Rb, and Rc fields always occur in the same place in an instruction to simplify decoding and keep the register read address which is needed prior to enqueue at a fixed decoding location. The Rt field is allowed to float around to make the instruction encoding easier. In a pipelined processor there is usually at least one clock cycle before Rt is used meaning it has time to be shifted around before it’s use.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Fields | | | | | | | | | | | |  |
|  | Immed16 | | | | | | | | Rt6 | Ra6 | | Opcode8 | RI |
|  | Immed16 | | | | | | | | Rt6 | Fn | On | Opcode8 | OI |
|  | Funct6 | | | | ~ | Sz3 | Rt6 | | Rb6 | Ra6 | | Opcode8 | R2 |
|  | 016 | | | | ~ | Sz3 | Funct6 | | Rt6 | Ra6 | | Opcode8 | R1 |
|  | Funct6 | | | | I | Sz3 | Rt6 | | Rb6 | Ra6 | | Opcode8 | SR |
|  | Funct6 | | | | I | Sz3 | Immed6 | | Rt6 | Ra6 | | Opcode8 | SI |
|  | Funct4 | | Me6 | | | | Mb6 | | Rt6 | Ra6 | | Opcode8 | BF |
|  | Disp13 | | | | | | | Cn3 | Rb6 | Ra6 | | Opcode8 | BD |
|  | Disp13 | | | | | | | Cn3 | Bitno6 | Ra6 | | Opcode8 | BB |
|  | Disp13 | | | | | | | Immed9 | | Ra6 | | Opcode8 | BI |
|  | ~4 | | P2 | | Cnd4 | | Rc6 | | Rb6 | Ra6 | | Opcode8 | BR |
|  | Funct5 | | | ar2 | | Sc3 | Rt6/Rc6 | | Rb6 | Ra6 | | Opcode8 | MX |
|  | Op2 | OL2 | Regno12 | | | | | | Rt6 | Ra6 | | Opcode8 | CS |
|  | Address28 | | | | | | | | | | | Opcode8 | JC |
|  | Funct5 | | | P2 | | Rm3 | Rt6 | | Rb6 | Ra6 | | Opcode8 | FP |
|  | Funct5 | | | T2 | | Vm3 | Rt6 | | Rb6 | Ra6 | | Opcode8 | VC |

There are a handful of additional formats primarily for control type instructions. See the particular instruction for the exact format used and additional information.

|  |  |
| --- | --- |
| Format | Instruction Group |
| RI | register-immediate and load / store with displacement |
| OI | register octant immediate |
| RR | register-register, two source registers |
| R1 | single source register |
| SR | shift register-register |
| SI | shift register-immediate |
| BF | bitfield |
| BD | branch with displacement |
| BB | branch on bit set / clear, decrement and branch |
| BI | branch equal immediate |
| BR | branch to register |
| MX | memory indexed |
| CS | control and status register access |
| JC | jump and call |
| FP | floating-point |
| VC | vector |

There are quite a few instructions operating on memory. Once volatile and non-volatile loads, stores, read-modify-write, and different sizes of operations are taken into consideration there are about 50 memory ops.

A single bit (bit 6 of the opcode) in the instruction determines if the instruction is a memory instruction or some other type of instruction. Memory instructions are further broken down into three groups – loads, stores, and read-modify-write instructions. Also, easily discernible by looking at the next two bits (bits 5 and 4) of the opcode.

## Compressed Register Specification

4 bit to 6 bit map

|  |  |  |  |
| --- | --- | --- | --- |
| Ra/Rt4 | Ra/Rt6 | Ra/Rt4 | Ra/Rt6 |
| 0 | 1 | 8 | 14 |
| 1 | 2 | 9 | 18 |
| 2 | 3 | 10 | 19 |
| 3 | 4 | 11 | 20 |
| 4 | 5 | 12 | 23 |
| 5 | 11 | 13 | 60 |
| 6 | 12 | 14 | 61 |
| 7 | 13 | 15 | 62 |

## ABS – Absolute Value

**Description:**

This instruction takes the absolute value of a register and places the result in a target register.

**Instruction Format:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 016 | ~3 | Sz3 | 46 | Rt6 | Ra6 | 02h8 |

**Clock Cycles:** 1

**Execution Units:** ALU #0 only

**Operation:**

If Ra < 0

Rt = -Ra

else

Rt = Ra

Exceptions: none

Notes:

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word |
| 4 | Byte Parallel |
| 5 | Char Parallel |
| 6 | Half Parallel |
| 7 | Word |

## ADD - Addition

Description:

Add two values. The first operand must be in a register. The second operand may be in a register or may be an immediate value specified in the instruction.

Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Immed16 | Rt6 | Ra6 | 04h8 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 046 | ~2 | Ov | Sz3 | Rt6 | Rb6 | Ra6 | 02h8 |

|  |  |
| --- | --- |
| Ov |  |
| 0 | no overflow |
| 1 | overflow exception if overflow occurred and enabled in AEC |

Overflow works properly only on 64 bit values.

Compressed Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| 0h4 | Immed6 | 2h2 | Ra/Rt61 |

1 Ra/Rt6 is not 0 (NOP) or 63 (ADDISP)

|  |  |  |  |
| --- | --- | --- | --- |
| 1h4 | Rb6 | 3h2 | Rt6 |

Rt = Rt + Rb

Instruction Format:

This format performs the ‘add’ operation with an immediate value to one of four quadrants of the target register. It may be used to build a 64 bit constant in a register. The immediate is sign extended to 64 bits then shifted by 0, 16, 32 or 48 bits to the left.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Immed16 | Rt6 | 13 | Q3 | 0Bh8 |

|  |  |
| --- | --- |
| Q3 | Bits |
| 0 | 0 to 15 |
| 1 | 16 to 31 |
| 2 | 32 to 47 |
| 3 | 48 to 63 |
| 4 to 7 | reserved |

**Clock Cycles:** 0.5

**Execution Units:** All ALU’s

Exceptions:

The immediate form of the instruction will not cause an exception. The registered form of the instruction may cause an overflow exception if enabled in the AEC register.

Notes:

For sub-word forms the part of the register updated corresponds to the size selected. For instance, if a byte operation is specified then only the low order eight bits of the target register is updated, the remaining bits hold their current value. For parallel operation forms the registers are treated as if they were a group of registers corresponding to the size selected. And the same operation is performed on each part of the register. For parallel forms the entire register is updated.

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word |
| 4 | Byte Parallel |
| 5 | Char Parallel |
| 6 | Half Parallel |
| 7 | Word |

## AND – Bitwise And

Description:

Perform a bitwise ‘and’ operation between operands.

Instruction Format:

The immediate value is sign extended on the left before use.

|  |  |  |  |
| --- | --- | --- | --- |
| Immed16 | Rt6 | Ra6 | 08h8 |

Rt = Ra & Rb

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 086 | ~3 | Sz3 | Rt6 | Rb6 | Ra6 | 02h8 |

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word1 |
| 4 | Byte Parallel1 |
| 5 | Char Parallel1 |
| 6 | Half Parallel1 |
| 7 | Word1 |

1 These codes are redundant with each other. They all have the same effect.

Compressed Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| 2h4 | Immed6 | 2h2 | Ra/Rt61 |

1Ra/Rt is non-zero.

The immediate value is sign extended on the left before use.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4h4 | 12 | Rb4 | 22 | 32 | Ra/Rt4 |

Rt = Rt & Rb

Instruction Format:

This format performs the ‘and’ operation with an immediate value to one of four quadrants of the target register. It may be used to build a 64 bit constant in a register. The immediate is shifted to the left by 0, 16, 32, or 48 bits then one extended on both the left and right sides. Note this instruction will only mask out bits in the selected quadrant.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Immed16 | Rt6 | 23 | O3 | 0Bh8 |

|  |  |
| --- | --- |
| O3 | Bits |
| 0 | 0 to 15 |
| 1 | 16 to 31 |
| 2 | 32 to 47 |
| 3 | 48 to 63 |
| 4 to 7 | reserved |

Clock Cycles: 0.5

**Execution Units: All** ALUs

**Exceptions:** none

## ASL – Arithmetic Shift Left

Description:

Shift left with arithmetic overflow exception. Bits from the source register Ra are shifted left by the amount in register Rb or an immediate value. A zero is shifted into bit zero. The difference between this instruction and a SHL instruction is that ASL may cause an arithmetic overflow exception. SHL will never cause an exception. In most cases the SHL instruction is preferred.

Instruction Format:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 11h6 | 0 | Sz3 | Rt6 | Rb6 | Ra6 | 02h8 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 11h6 | 1 | Sz3 | Imm6 | Rb6 | Ra6 | 02h8 |

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word1 |
| 4 | Byte Parallel1 |
| 5 | Char Parallel1 |
| 6 | Half Parallel1 |
| 7 | Word1 |

Compressed Instruction Format:

There is no compressed instruction format for this instruction. See SHL for a compressed version of the left shift instruction.

Clock Cycles: 1

**Execution Units:** ALU #0 Only

Exceptions:

An overflow exception may result if the bits shifted out from the MSB are not the same as the resulting sign bit and the exception is enabled in the AEC register. Exceptions are only caused by a word size operation.

## DBNZ –Decrement, Branch if Not Zero

Description:

If the specified register is non-zero then an thirteen bit sign extended value is added to the program counter. The branch is relative to the address of the instruction directly following the branch. The register is also decremented by one.

Instruction Format:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 35 23 | 22 20 | 19 14 | 13 8 | 7 0 |
| Displacement13 | 73 | 06 | Ra6 | 3Ch8 |

Operation:

if (Ra<>0)

pc = pc + displacement

Ra = Ra - 1

Clock Cycles: 1

**Execution Units:** FCU Only

Exceptions: none

## LDI – Load Immediate

Description:

This instruction loads an immediate value into a register. It is an alternate mnemonic for the OR instruction.

Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Immed16 | Rt6 | 06 | 09h8 |

Instruction Format:

This format performs the ‘ldi’ operation with an immediate value to one of eight octants of the target register. It may be used to build a 128 bit constant in a register. The immediate constant is zero extended then shifted to the left by a multiple of 16 bits.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Immed16 | Rt6 | 43 | O3 | 0Bh8 |

|  |  |
| --- | --- |
| O3 | Bits |
| 0 | 0 to 15 |
| 1 | 16 to 31 |
| 2 | 32 to 47 |
| 3 | 48 to 63 |
| 4 to 7 | reserved |

Clock Cycles: 0.5

## OR – Bitwise Or

Description:

Perform a bitwise or operation between operands.

Instruction Format:

The immediate value is sign extended to the left before use.

Rt = Ra | immed

|  |  |  |  |
| --- | --- | --- | --- |
| Immed16 | Rt6 | Ra6 | 09h8 |

Rt = Ra | Rb

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 096 | ~3 | Sz3 | Rt6 | Rb6 | Ra6 | 02h8 |

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word1 |
| 4 | Byte Parallel1 |
| 5 | Char Parallel1 |
| 6 | Half Parallel1 |
| 7 | Word1 |

1 These codes are redundant with each other. They all have the same effect.

Compressed Instruction Format:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4h4 | Immed6 | 2h2 | 2h2 | Ra/Rt4 |

The immediate value is sign extended on the left before use.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4h4 | 22 | Rb4 | 22 | 32 | Ra/Rt4 |

Rt = Rt | Rb

|  |  |  |  |
| --- | --- | --- | --- |
| Ra/Rt4 | Ra/Rt6 | Ra/Rt4 | Ra/Rt6 |
| 0 | 1 | 8 | 14 |
| 1 | 2 | 9 | 18 |
| 2 | 3 | 10 | 19 |
| 3 | 4 | 11 | 20 |
| 4 | 5 | 12 | 23 |
| 5 | 11 | 13 | 60 |
| 6 | 12 | 14 | 61 |
| 7 | 13 | 15 | 62 |

Instruction Format:

This format performs the ‘or’ operation with an immediate value to one of eight octants of the target register. It may be used to build a 128 bit constant in a register. The immediate constant is zero extended then shifted to the left by a multiple of 16 bits.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Immed16 | Rt6 | 03 | O3 | 0Bh8 |

|  |  |
| --- | --- |
| O3 | Bits |
| 0 | 0 to 15 |
| 1 | 16 to 31 |
| 2 | 32 to 47 |
| 3 | 48 to 63 |
| 4 to 7 | reserved |

Clock Cycles: 0.5

**Execution Units: All** ALUs

Exceptions: none

## RET – Return from Subroutine

Description:

This instruction performs a subroutine return by loading the program counter with the contents of the return address register. Additionally, the stack pointer is adjusted by a constant supplied in the instruction. The immediate constant should be a multiple of eight to keep the stack word aligned.

Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Immed16 | 3Dh6 | 3Fh6 | 32h8 |

PC = RA

SP = SP + Immediate

Compressed Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| 2h4 | Immed6 | 2h2 | 06 |

For this format, the immediate constant is shifted left three times and zero extended before use.

Clock Cycles: 1

Exceptions: none

Notes:

## SHL – Shift Left

Description:

Bits from the source register Ra are shifted left by the amount in register Rb or an immediate value. A zero is shifted into bit zero. The difference between this instruction and an ASL instruction is that ASL may cause an arithmetic overflow exception. SHL will never cause an exception. SHL also has a compressed instruction form which ASL does not.

Instruction Format:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 10h6 | 0 | Sz3 | Rt6 | Rb6 | Ra6 | 02h8 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 10h6 | 1 | Sz3 | Imm6 | Rb6 | Ra6 | 02h8 |

Compressed Instruction Format:

|  |  |  |  |
| --- | --- | --- | --- |
| 3h4 | Immed6 | 2h2 | Ra/Rt6 |

|  |  |
| --- | --- |
| Sz3 |  |
| 0 | Byte |
| 1 | Char |
| 2 | Half |
| 3 | Word1 |
| 4 | Byte Parallel1 |
| 5 | Char Parallel1 |
| 6 | Half Parallel1 |
| 7 | Word1 |

Clock Cycles: 1

**Execution Units:** ALU #0 Only

Exceptions: none

## Compressed Instruction Formats

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | |  |  | |  |
| 0000 | | 006 | | 10 | 06 | | NOP |
| 0000 | | Amt[8..3] | | 10 | 636 | | ADDISP |
| 0000 | | Amt6 | | 10 | Ra/Rt6 | | ADDI |
| 0001 | | Amt6 | | 10 | Rt6 | | LDI / SYS (SYS if Rt = 0) |
| 0010 | | Amt6 | | 10 | Ra/Rt6 | | RET / ANDI (RET if Ra=0) |
| 0011 | | Amt6 | | 10 | Rt6 | | SHLI |
| 0100 | | Amt6 | | 10 | 00 | Ra/Rt’4 | SHRI |
| 0100 | | Amt6 | | 10 | 01 | Ra/Rt’4 | ASRI |
| 0100 | | Amt6 | | 10 | 10 | Ra/Rt’4 | ORI |
| 0100 | | 00 | Rb’4 | 10 | 11 | Ra/Rt’4 | SUB |
| 0100 | | 01 | Rb’4 | 10 | 11 | Ra/Rt’4 | AND |
| 0100 | | 10 | Rb’4 | 10 | 11 | Ra/Rt’4 | OR |
| 0100 | | 11 | Rb’4 | 10 | 11 | Ra/Rt’4 | XOR |
| 0101 | | Address11..6 | | 10 | Address5..0 | | CALL |
| 0110 | |  | | 10 |  | | reserved |
| 0111 | | Disp11..6 | | 10 | Disp5..0 | | BRA |
| 10 | Disp8 | | | 10 | Ra6 | | BEQZ |
| 11 | Disp8 | | | 10 | Ra6 | | BNEZ |
| 0000 | | Rt6 | | 11 | Ra6 | | MOV |
| 0001 | | Rb6 | | 11 | Ra/Rt6 | | ADD |
| 0010 | | Rt6 | | 11 | Ra6 | | JALR |
| 0011 | | ?????? | | 11 | Ra6 | | reserved |
| The following two instructions have SP as an implied register read | | | | | | | |
| 0100 | | Disp7..2 | | 11 | Rt6 | | LH Rt,d[SP} |
| 0101 | | Disp8..3 | | 11 | Rt6 | | LW Rt,d[SP] |
| The following two instructions have FP as an implied register read | | | | | | | |
| 0110 | | Disp7..2 | | 11 | Rt6 | | LH Rt,d[FP] |
| 0111 | | Disp8..3 | | 11 | Rt6 | | LW Rt,d[FP] |
| The following two instructions have SP as an implied register read | | | | | | | |
| 1000 | | Disp7..2 | | 11 | Rb6 | | SH Rb,d[SP] |
| 1001 | | Disp8..3 | | 11 | Rb6 | | SW Rb,d[SP] |
| The following two instructions have FP as an implied register read | | | | | | | |
| 1010 | | Disp7..2 | | 11 | Rb6 | | SH Rb,d[FP] |
| 1011 | | Disp8..3 | | 11 | Rb6 | | SW Rb,d[FP] |
| 1100 | | d5..4 | Rt’4 | 11 | d3..2 | Ra’4 | LH Rt,d[Ra] |
| 1101 | | d6..5 | Rt’4 | 11 | d4..3 | Ra’4 | LW Rt,d[Ra] |
| 111? | | d5..4 | Rb’4 | 11 | d3..2 | Ra’4 | SH Rb,d[Ra] |
| 1111 | | d6..5 | Rb’4 | 11 | d4..3 | Ra’4 | SW Rb,d[Ra] |

Several instructions may not be compressed due to format or other hardware limitations. In particular the vector instructions and branch on bit set/clear, and branch equal to immediate instructions may not be compressed.

Compressed instructions must follow the formats in this table. ‘?’ indicates where the bit(s) use may be defined by the application. Bits 8 to 11 (the register spec field) may also be defined by the application. It may be desirable in some cases to use these bits for immediate constants rather than a register spec. Bits 4 to 6 and 8 to 17 are used as a 13 bit index into a lookup table for the decompressed instruction.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Fmt | # Insn | 17 14 | | | 13 8 | | 7 6 | 5 0 | |  | Sample Insn |
| CA | 3 | 00?? | | | ?? | ?/Rb’4 | 10 | Ra/Rt6 | |  | nop, addi, shli |
| CB | 2 | 0001 | | | ?? | ?/Rb’4 | 10 | Rt6 | |  | ldi |
| CC | 3 | 0100 | | | ?? | ?/Rb’4 | 10 | ?? | Ra/Rt’4 |  | shri, asri andi |
| CD | 4 | 0100 | | | ?? | ?/Rb’4 | 10 | 11 | Ra/Rt’4 |  | sub, and, or, xor |
| CE |  | 0101 | | |  |  | 10 |  |  | reserved |  |
| CF |  | 0110 | | |  |  | 10 |  |  | reserved |  |
| CG | 1 | 0111 | | | ?? | ?/Rb’4 | 10 | ?? | Ra’4 | ? = Displacement bit | bra |
| CH | 2 | 1 | ????? | | | ?/Rb’4 | 10 | Ra6 | | ? = Displacement bit | beqz bnez |
| CI | 4 | 00?? | | | Rt6 | | 11 | Ra6 | | 1 Full Read Port, 1 Full Write Port | mov add jalr |
| CJ | 2+ | 010 | | ??? | | ?/Rb’4 | 11 | Rt6 | | SP implied | lw Rt, d[SP] |
| CK | 2+ | 011 | | ??? | | ?/Rb’4 | 11 | Rt6 | | FP implied | lw Rt, d[FP] |
| CL | 2+ | 100 | | ??? | | ???? | 11 | Rb6 | | SP implied, 2nd Read port | sw Rb, d[SP] |
| CM | 2+ | 101 | | ??? | | ???? | 11 | Rb6 | | FP implied, 2nd read port | sw Rb, d[FP] |
| CN | 2+ | 110 | | ??? | | ?/Rt’4 | 11 | ?? | Ra’4 | 1 read port | lw Rt, d[Ra] |
| CO | 2++ | 111 | | ??? | | ?/Rb’4 | 11 | ?? | Ra’4 | 2 read ports | sw Rb, d[Ra] |

It is assumed that registers r32 to r63 will be used primarily for floating point and registers r0 to r31 for integer values.

To conserve space not all the bits of the decompressed instruction are stored. Only the following bits are needed in the decompression table: opcode bits 0 to 6 and instruction bits 14 to 35. Bit 7 is always a 1 for decompressed instructions so doesn’t need to be stored in the table. Bits 8 to 13 represent the register file address bits which are not required in the table as they are inserted from the decompressed instruction.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 35 20 | 19 14 | 13 8 | 7 | 6 0 |
| Other16 | Rt/Rb6 | Ra6 | 1 | Opcode7 |

## Major Opcode (inst. bits 0 to 6)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | x0 | x1 | x2 | x3 | x4 | x5 | x6 | x7 | x8 | x9 | xA | xB | xC | xD | xE | xF |
| 0x |  | {VECTOR} | {R2} |  | ADDI |  | CMPI | CMPUI | ANDI | ORI | XORI | QOPI | EXEC | FMA | CSR | {FLOAT} |
| 1x |  |  |  |  |  |  | {Bitfield} | {Bitfield} | MULI | MULUI | MULSUI | FNMS | DIVI | DIVUI | DIVSUI | FMS |
| 2x | SEQI | SNEI | SLTI | SGEI | SLEI | SGTI | SLTUI | SGEUI | SLEUI | SGTUI | CACHE |  | MODI | MODUI | MODSUI | FNMA |
| 3x | JMP | CALL | RET | JAL | SYS | REX |  |  | Bcc | BccR |  |  | BBc | BEQ# | FBcc | FBccR |
| 4x | LB | LBU | LBO | LC | LCU | LCO | LH | LHU | LHO | LW | LWU | LWO | LQ | {Indexed Load} | LV |  |
| 5x | LVB | LVBU | LVBO | LVC | LVCU | LVCO | LVH | LVHU | LVHO | LVW | LVWU | LVWO | LVQ | LVWR | LVV |  |
| 6x | SB | SC | SH | SW | SQ | SWC | SV | {Indexed} |  |  |  |  |  |  |  |  |
| 7x | ASWAP | AADD | AAND | AOR | AXOR | AMIN | AMAX | AMINU | AMAXU | ASHL | ASHR | INC |  |  |  |  |

## {R2} Major Func (inst. bits 30 to 35)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | x0 | x1 | x2 | x3 | x4 | x5 | x6 | x7 | x8 | x9 | xA | xB | xC | xD | xE | xF |
| 0x | {BCD} | {R1} |  |  | ADD | SUB | CMP | CMPU | AND | OR | XOR |  | NAND | NOR | XNOR |  |
| 1x | SHL | ASL | SHR | ASR | ROL | ROR |  |  | MUL | MULU | MULSU | MOV | DIV | DIVU | DIVSU |  |
| 2x | SEQ | SNE | SLT | SGE | SLE | SGT | SLTU | SGEU | SLEU | SGTU | CACHEX |  | MOD | MODU | MODSU |  |
| 3x |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

## {Indexed Load} Major Func (inst. bits 31 to 35)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | x0 | x1 | x2 | x3 | x4 | x5 | x6 | x7 | x8 | x9 | xA | xB | xC | xD | xE | xF |
| 0x | LBX | LBUX | LBOX | LCX | LCUX | LCOX | LHX | LHUX | LHOX | LWX | LWUX | LWOX | LQX |  | LVX |  |
| 1x | LVBX | LVBUX | LVBOX | LVCX | LVCUX | LVCOX | LVHX | LVHUX | LVHOX | LVWX | LVWUX | LVWOX | LVQX | LVWRX | LVVX |  |

## {Indexed} Major Func (inst. bits 31 to 35)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | x0 | x1 | x2 | x3 | x4 | x5 | x6 | x7 | s8 | x9 | xA | xB | xC | xD | xE | xF |
| 0x | SBX | SCX | SHX | SWX | SQX | SWCX | SVX |  |  |  |  |  |  |  |  |  |
| 1x | ASWAPX | AADDX | AANDX | AORX | AXORX | AMINX | AMAXX | AMINUX | AMAXUX | ASHLX | ASHRX | INCX |  |  |  |  |