Gambit

# Overview

Gambit is a superscalar processor with a 52-bit native operating mode. Native mode makes use of a 32-entry register file. Native mode instructions vary in length up to 52-bits. The processor manages branching using a compare instruction and status flags results.

# Programming Model

## General Registers

|  |  |  |  |
| --- | --- | --- | --- |
| Reg |  |  | Usage |
| R0 | z | This register is always zero |  |
| R1 | acc | Accumulator | First parameter / return value / loop count |
| R2 | x | ‘x’ index register | Second parameter |
| R3 | y | ‘y’ index register | Third parameter |
| R4 |  |  |  |
| R5 |  |  |  |
| R6 |  |  |  |
| R7 to 29 |  |  |  |
| R30 | fp | frame pointer |  |
| R31 | sp | stack pointer |  |
|  |  |  |  |
| SR | sr | status register | conditional branching |

## Memory Addressing

The cpu is word oriented with byte addressable memory. The smallest addressable unit of data is a 13-bit byte. Up to 252 Bytes of data are supported and 252 bytes of code.

# Instruction Set Summary

The instruction set includes basic arithmetic, logic, and shift instructions including: add, sub, and, or, eor, asl, rol, lsr, and ror. There are several additional instructions which are alternate mnemonics for other instructions. These include bit, and cmp.

The cycle counts are assuming no wait states are required for either instructions or data and both instructions and data can be found in the cache.

# ALU Operations

## ADD – Addition

**Description**:

Add two operand values and place the result in the target register, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: v c n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## AND – Bitwise ‘And’

**Description**:

Bitwise ‘And’ two operand values and place the result in the target register, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value. The AND instruction has an alternate mnemonic called BIT which updates the flags slightly differently.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## ASL – Arithmetic Shift Left

**Description**:

Left shift one operand value by a second operand value and place the result in the target register, updating status flags. Zeros are shifted into the least significant bits. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## BIT – Bitwise ‘And’

**Description**:

Bitwise ‘And’ two operand values and discard the result, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value. The BIT instruction is an alternate mnemonic for the AND instruction where the target register is specified as R0. The BIT instruction updates the overflow flag to the status of bit 50 of the result.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: v n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## CMP – Comparison

**Description**:

Subtract two operand values and discard the result, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value. The CMP instruction is an alternate mnemonic for the SUB instruction when the target register is R0. However, unlike SUB, CMP does not update the overflow flag.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: c n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## EOR – Bitwise Exclusive ‘Or’

**Description**:

Bitwise exclusive ‘Or’ two operand values and place the result in the target register, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## LSR – Logical Shift Right

**Description**:

Right shift one operand value by a second operand value and place the result in the target register, updating status flags. Zeros are shifted into the most significant bits. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## OR – Bitwise ‘Or’

**Description**:

Bitwise ‘Or’ two operand values and place the result in the target register, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## ROL – Rotate Left

**Description**:

Rotate left one operand value by a second operand value and place the result in the target register, updating status flags. The most significant bits are placed in the least significant bits. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## ROR – Rotate Right

**Description**:

Rotate right one operand value by a second operand value and place the result in the target register, updating status flags. The least significant bits are placed in the most significant bits. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value.

**Formats Supported**: RR, RI9

**Flags Affected**: n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

## SUB – Subtraction

**Description**:

Subtract two operand values and place the result in the target register, updating status flags. The first operand must be in a register specified by the Ra5 field of the instruction. The second operand may be either a register specified by the Rb5 field of the instruction, or an immediate value. The subtraction instruction has an alternate mnemonic CMP which updates the flags differently when the target register is R0.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: v c n z

**Execution Units**: ALU

**Clock Cycles**: 0.5

**Exceptions**: none

# Memory Operations

## LD – Load Data (52 bits)

**Description**:

Data is loaded from the memory address which is either the sum of Ra and an immediate value or the sum of Ra and Rb. Both register indirect with displacement and indexed addressing are supported.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: n z

**Operation:**

Rt = Memory52[d+Ra]

or

Rt = Memory52[Ra+Rb]

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## LDB – Load Data Byte (13 bits)

**Description**:

Data is loaded from the memory address which is the sum of Ra and an immediate value. Only register indirect with displacement addressing is supported.

**Formats Supported**: RI36

**Flags Affected**: n z

**Operation:**

Rt = Memory13[d+Ra]

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## PHP – Push Processor Status to Stack (52 bits)

**Description**:

The stack pointer is decremented then the status register is stored to the memory address which is contained in the stack pointer register (R31).

**Formats Supported**: PHP

**Flags Affected**: none

**Operation:**

SP = SP - 4

Memory13[SP] = SR

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## PLP – Pull Processor Flags from Stack (52 bits)

**Description**:

The status register is loaded from the memory address which is contained in the stack pointer register (R31) into a general-purpose register. Then the stack pointer is incremented.

**Formats Supported**: PLP

**Flags Affected**: c v n z i u

**Operation:**

Rt = Memory13[SP]

SP = SP + 4

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## POP – Pop Data from Stack (52 bits)

**Description**:

Data is loaded from the memory address which is contained in the stack pointer register (R31) into a general purpose register. Then the stack pointer is incremented.

**Formats Supported**: POP

**Flags Affected**: n z

**Operation:**

Rt = Memory13[SP]

SP = SP + 4

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## PSH – Push Data to Stack (52 bits)

**Description**:

The stack pointer is decremented then data from a general-purpose register is stored to the memory address which is contained in the stack pointer register (R31).

**Formats Supported**: PSH

**Flags Affected**: none

**Operation:**

SP = SP - 4

Memory13[SP] = Rs

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## ST – Store Data (52 bits)

**Description**:

Data is stored to the memory address which is either the sum of Ra and an immediate value or the sum of Ra and Rb. Both register indirect with displacement and indexed addressing are supported.

**Formats Supported**: RR, RI9, RI23, RI36

**Flags Affected**: none

**Operation:**

Memory52[d+Ra] = Rs

or

Memory52[Ra+Rb] = Rs

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

## STB – Store Data Byte (13 bits)

**Description**:

Data is stored to the memory address which is the sum of Ra and an immediate value. Only register indirect with displacement addressing is supported.

**Formats Supported**: RI36

**Flags Affected**: none

**Operation:**

Memory13[d+Ra] = Rs

or

Memory13[Ra+Rb] = Rs

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

# Flow Control (Branch Unit) Operations

## JMP – Jump

**Description**:

Transfer execution of instructions to the address specified by the instruction. The target address may be either a 46-bit absolute address or an address contained in a register. For absolute address mode only the low order 46 bits of the program counter are affected. The upper six bits of the program counter remain the same.

**Formats Supported**: ABS46, R

**Flags Affected**: none

**Operation:**

PC = Address46

or

PC = Ra

**Execution Units**: Mem

**Clock Cycles**: 1

**Exceptions**: none

## JSR – Jump to Subroutine

**Description**:

Push the address of the next instruction on the stack, then transfer execution of instructions to the address specified by the instruction. The target address may be either a 46-bit absolute address or an address contained in a register. For absolute address mode only the low order 46 bits of the program counter are affected. The upper six bits of the program counter remain the same.

**Formats Supported**: ABS46, R

**Flags Affected**: none

**Operation:**

SP = SP – 4

Memory52[SP] = Next PC

PC = Address46

or

PC = Ra

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

**Notes**:

The next PC is either the current PC plus four when absolute addressing is used, or the current PC plus one if register indirect addressing is used.

## RTI – Return from Interrupt Subroutine

**Description**:

Pop the status register from the stack. Next pop the address to return to from the stack, then transfer execution of instructions to that address.

**Formats Supported**: RTI

**Flags Affected**: none

**Operation:**

SR = Memory52[SP]

SP = SP + 4

PC = Memory52[SP]

SP = SP + 4

**Execution Units**: Mem

**Clock Cycles**: 8 if data is in the cache.

**Exceptions**: none

**Notes**:

## RTS – Return from Subroutine

**Description**:

Pop the address of the next instruction from the stack, then transfer execution of instructions to that address.

**Formats Supported**: RTS

**Flags Affected**: none

**Operation:**

PC = Memory52[SP]

SP = SP + 4

**Execution Units**: Mem

**Clock Cycles**: 4 if data is in the cache.

**Exceptions**: none

**Notes**:

# Instruction Formats

## Arithmetic / Logical

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ADD | Flags: v c n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | Rt5 | 00o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | Rt5 | 00o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | Rt5 | 01o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | Rt5 | 02o | ADD Rt,Ra,#imm30 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SUB | Flags: v c n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | Rt5 | 10o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | Rt5 | 10o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | Rt5 | 11o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | Rt5 | 12o | ADD Rt,Ra,#imm30 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| CMP | Flags: c n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | 05 | 10o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | 05 | 10o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | 05 | 11o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | 05 | 12o | ADD Rt,Ra,#imm30 | 4 |

CMP is an alternate mnemonic for SUB where the target register is R0. CMP does not alter the overflow flag.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| AND | Flags: n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | Rt5 | 30o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | Rt5 | 30o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | Rt5 | 31o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | Rt5 | 32o | ADD Rt,Ra,#imm30 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| BIT | Flags: v n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | 05 | 30o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | 05 | 30o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | 05 | 31o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | 05 | 32o | ADD Rt,Ra,#imm30 | 4 |

Bit is the AND operation with no target register; the overflow status is set to bit 50 of the result

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| OR | Flags: n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | Rt5 | 40o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | Rt5 | 40o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | Rt5 | 41o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | Rt5 | 42o | ADD Rt,Ra,#imm30 | 4 |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EOR | Flags: n z | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | Rb5 | Ra5 | Rt5 | 50o | ADD Rt,Ra,Rb | 2 |
|  | | | 1 | Imm9 | | Ra5 | Rt5 | 50o | ADD Rt,Ra,#imm6 | 2 |
|  | | Imm23 | | | | Ra5 | Rt5 | 51o | ADD Rt,Ra,#imm14 | 3 |
| Imm36 | | | | | | Ra5 | Rt5 | 52o | ADD Rt,Ra,#imm30 | 4 |

## Shift Operations / Read-modify-write memory operations.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ASL | Flags: c n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | | Rb5 | Ra5 | Rt5 | 06o | Rt,Ra,Rb | 2 |
|  | | | 1 | ~3 | Imm6 | | Ra5 | Rt5 | 06o | Rt,Ra,#imm10 | 2 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ROL | Flags: c n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | | Rb5 | Ra5 | Rt5 | 16o | Rt,Ra,Rb | 2 |
|  | | | 1 | ~3 | Imm6 | | Ra5 | Rt5 | 16o | Rt,Ra,#imm10 | 2 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LSR | Flags: c n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | | Rb5 | Ra5 | Rt5 | 26o | Rt,Ra,Rb | 2 |
|  | | | 1 | ~3 | Imm6 | | Ra5 | Rt5 | 26o | Rt,Ra,#imm10 | 2 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ROR | Flags: c n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 21 | | | 20 16 | 15 11 | 10 6 | 5 0 |  |  |
|  | |  | 0 | ~4 | | Rb5 | Ra5 | Rt5 | 36o | Rt,Ra,Rb | 2 |
|  | | | 1 | ~3 | Imm6 | | Ra5 | Rt5 | 36o | Rt,Ra,#imm10 | 2 |

## Load and Store Instructions

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LD | Flags: n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | | 25 16 | | | 15 11 | 10 6 | 5 0 |  |  |
|  | | | 0 | | ~4 | Rb5 | Ra5 | Rt5 | 60o | Rt.[Ra+Rb] | 2 |
|  | | | 1 | | Disp9 | | Ra5 | Rt5 | 60o | Rt,d9[Ra] | 2 |
|  | | Disp23 | | | | | Ra5 | Rt5 | 61o | Rt,d23[Ra] | 3 |
| Addr36 | | | | | | | Ra5 | Rt5 | 62o | Rt,d36[Ra] | 4 |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| LDB | Flags: n z | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 16 | 15 11 | 10 6 | 5 0 |  |  |
| Addr36 | | | | Ra5 | Rt5 | 64o | Rt,d[Ra] | 4 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ST | Flags: n z | | | | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | | 25 16 | | | 15 11 | 10 6 | 5 0 |  |  |
|  | | | 0 | | ~4 | Rb5 | Ra5 | Rs5 | 70o | Rs.[Ra+Rb] | 2 |
|  | | | 1 | | Disp9 | | Ra5 | Rs5 | 70o | Rs,d9[Ra] | 2 |
|  | | Disp23 | | | | | Ra5 | Rs5 | 71o | Rs,d23[Ra] | 3 |
| Addr36 | | | | | | | Ra5 | Rs5 | 72o | Rs,d36[Ra] | 4 |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| STB | Flags: | | | | | Opcode |  | Bytes |
| 51 39 | | 38 26 | 25 16 | 15 11 | 10 6 | 5 0 |  |  |
| Addr36 | | | | Ra5 | Rs5 | 74o | Ra,d[Ra] | 4 |

## Flow Control

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JMP | Flags: | | | | | | Bytes |
|  | | Address46 | | | 04o | JMP abs46 | 4 |
|  | | | ~2 | Ra5 | 44o | JMP [Ra] | 1 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JSR | Flags: | | | | | | Bytes |
|  | | Address46 | | | 14o | JSR abs46 | 4 |
|  | | | ~2 | Ra5 | 54o | JSR [Ra] | 1 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| RTS | Flags: | ~4 | 0 | 24o | RTS | 1 |
| RTI | Flags: z n c v b d i u | ~4 | 1 | 24o | RTI | 1 |
| PFI | Flags: | ~4 | 2 | 24o | PFI | 1 |
| WAI | Flags: | ~4 | 4 | 24o | WAI | 1 |
| STP | Flags: | ~4 | 6 | 24o | STP | 1 |
| NOP | Flags: | ~4 | 7 | 24o | NOP | 1 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| BEQ | Flags: | Disp17 | 0 | 15o | BEQ disp | 2 |
| BNE | Flags: | Disp17 | 1 | 05o | BNE disp | 2 |
| BPL | Flags: | Disp17 | 2 | 05o | BPL disp | 2 |
| BMI | Flags: | Disp17 | 3 | 05o | BMI disp | 2 |
| BVS | Flags: | Disp17 | 4 | 05o | BVS disp | 2 |
| BVC | Flags: | Disp17 | 5 | 05o | BVC disp | 2 |
| BCS | Flags: | Disp17 | 6 | 05o | BCS disp | 2 |
| BCC | Flags: | Disp17 | 7 | 05o | BCC disp | 2 |
| BRA | Flags: | Disp17 | 0 | 25o | BRA disp | 2 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| RST | Flags: b | ~4 | 0 | 34o | RST | 1 |
| NMI | Flags: b | ~4 | 1 | 34o | NMI | 1 |
| IRQ | Flags: b | ~4 | 2 | 34o | IRQ | 1 |
| BRK | Flags: b | Const4 | 3 | 34o | BRK | 1 |

## Stack push and pop operations.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PHP | Flags: | ~7 | | 75o | PHP | 1 |
| PSH | Flags: | ~2 | Ra5 | 76o | PSH Ra | 1 |
| PLP | Flags: z c v n i b d u | ~7 | | 65o | PLP | 1 |
| POP | Flags: n z | ~2 | Rt5 | 66o | POP Rt | 1 |

## Status Register Operations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| REP | Flags: c v n z i u | Mask7 | 56o | REP | 1 |
| SEP | Flags: c v n z i u | Mask7 | 46o | SEP | 1 |

## String Operations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| MVNB | Flags: | ~4 | 0 | 45o | MVN | 1 |
| MVPB | Flags: | ~4 | 1 | 45o | MVP | 1 |
| STSB | Flags: | ~4 | 2 | 45o | STS | 1 |
| CMPSB | Flags: c n z | ~4 | 3 | 45o | CMPS | 1 |
| MVN | Flags: | ~4 | 4 | 45o | MVN | 1 |
| MVP | Flags: | ~4 | 5 | 45o | MVP | 1 |
| STS | Flags: | ~4 | 6 | 45o | STS | 1 |
| CMPS | Flags: c n z | ~4 | 7 | 45o | CMPS | 1 |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

# Opcode Maps

## Root Level

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | xxx000 | xxx001 | xxx010 | xxx011 | xxx100 | xxx101 | xxx110 | xxx111 |
| 000xxx | ADD 2r,i9 | ADD 2r,i23 | ADD 2r,i36 |  | JMP |  | ASL 2r,i6 |  |
| 001xxx | SUB / CMP | SUB / CMP | SUB / CMP |  | JSR | Bcc d17 | LSR 2r,i6 |  |
| 010xxx |  |  |  |  | RTS / RTI |  | ROL 2r,i6 |  |
| 011xxx | AND / BIT | AND / BIT | AND / BIT |  | BRK | Bcc d17 | ROR 2r,i6 |  |
| 100xxx | OR | OR | OR |  | JMP [Rn] | {string} | SEP |  |
| 101xxx | EOR | EOR | EOR |  | JSR [Rn] |  | REP |  |
| 110xxx | LD | LD | LD |  | LDB | PLP | POP |  |
| 111xxx | ST | ST | ST |  | STB | PHP | PSH |  |

# Appendix

The first nine bits of the instruction are used as a nine-bit index into a table which holds pointers to micro-instructions.

## Micro-op Instruction Format

Micro-instructions are 24 bits in size.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| FL2 | Opcode6 | Cnst4 | Src24 | Src14 | Tgt4 |

FL2 are two bits holding the first / last micro-instruction indicators. 00 = middle instruction, 01 = first, 10 = last, 11 = first and last.

## Micro-op Fields

|  |  |
| --- | --- |
| Tgt4 | Meaning |
| 0 | The value 0 |
| 1 | Get from instruction bits 6 to 10 |
| 2 | The accumulator register |
| 3 | The X register |
| 4 | The Y Register |
| 5 | The stack pointer |
| 6 | the tmp1 register |
| 7 | the tmp2 register |
| 8 | the SR register |
| 9 | the PC register (source) |
| 10 | PC + 1 |
| 11 | PC + 4 |

|  |  |
| --- | --- |
| Src14 | Meaning |
| 0 | The value 0 |
| 1 | Get from register spec instruction bits 11 to 15 |
| 2 | The accumulator register |
| 3 | The X register |
| 4 | The Y Register |
| 5 | The stack pointer |
| 6 | the tmp1 register |
| 7 | the tmp2 register |
| 8 | the SR register |

|  |  |
| --- | --- |
| Src24 | Meaning |
| 0 | The value 0 |
| 1 | Get from register spec instruction bits 16 to 25 |
| 2 | The accumulator register |
| 3 | The X register |
| 4 | The Y Register |
| 5 | The stack pointer |
| 6 | the tmp1 register |
| 7 | the tmp2 register |
| 8 | the SR register |
| 9 | the value 1 |
| 11 |  |
| 15 | the value -1 |

|  |  |
| --- | --- |
| Cnst4 | Meaning |
| 0 | the value 0 |
| 1 | the value 1 |
| 2 | the value 2 |
| 3 | the value 3 |
| 4 | the value 4 |
| 5 | bits 9 to 25 |
| 6 | bits 9 to 12 (branches) |
| 7 | bits 6 to 51 ( JMP / JSR) |
| 8 | bits 16 to 25 of instruction |
| 9 | bits 16 to 38 of instruction |
| 10 | bits 16 to 51 of instruction |
| 11 | bits 6 to 12 (REP / SEP) |
| 13 | the value -3 |
| 14 | the value -2 |
| 15 | the value -1 |

Micro-op Lists for Instructions

BRK

SUB SP,SP,#4

ST PC+1,[SP]

SUB SP,SP,#4

ST FLAGS,[SP]

SEP #i

LD TMP,$FFFFFFFFFFFFC

JMP 0[TMP]

MVN

LD tmp,[X]

ST tmp,[Y]

ADD X,X,4

ADD Y,Y,4

SUB AC,AC,#1

BNE PC

MVP

LD tmp,[X]

ST tmp,[Y]

SUB X,X,#4

SUB Y,Y,#4

SUB AC,AC,#1

BNE PC

STS

ST X,[Y]

ADD Y,Y,#4

SUB AC,AC,#1

BNE PC

CMPS

LD tmp1,[X]

LD tmp2,[Y]

ADD X,X,#4

ADD Y,Y,#4

SUB ac,ac,#1

BEQ PC+1

CMP tmp1,tmp2

BEQ PC

## Micro-Instruction Opcodes

|  |  |  |
| --- | --- | --- |
| Opc6 |  | Flags Updated |
| 0 | ADD | - |
| 1 | ADD. | c v n z |
| 2 | SUB | - |
| 3 | SUB. | c v n z |
| 4 | AND. | n z |
| 5 | OR. | n z |
| 6 | EOR. | n z |
| 7 | LD | - |
| 8 | LD. | n z |
| 9 | LB | - |
| 10 | LB. | n z |
| 11 | ST | - |
| 12 | STB | - |
| 13 | ASL. | c n z |
| 14 | ROL. | c n z |
| 15 | LSR. | c n z |
| 16 | ROR. | c n z |
| 17 | BRA | - |
| 18 | BEQ | - |
| 19 | BNE | - |
| 20 | BMI | - |
| 21 | BPL | - |
| 22 | BCS | - |
| 23 | BCC | - |
| 24 | BVS | - |
| 25 | BVC | - |
| 26 | SEP | c v n z i u |
| 27 | REP | c v n z i u |
| 28 | JMP |  |
| 29 | STP |  |
| 30 | WAI |  |
| 31 |  |  |